|  |  |
| --- | --- |
| Hyundai Bayon | Technical Specifications\* |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Engines & performance  | 1.2 MPi 84 PS | 1.0 T-GDi 100 PS  | 1.0 T-GDi 100 PS 48V  | 1.0 T-GDi 120 PS 48V  |
| Emission standard | EURO 6d  | EURO 6d | EURO 6d | EURO 6d |
| Type  | 4 Cylinder MPi gasoline | 3 Cylinder Turbo GDi gasoline | 3 Cylinder Turbo GDi gasoline with 48V mild hybrid system | 3 Cylinder Turbo GDi gasoline with 48V mild hybrid system |
| Displacement [cc] | 1197 | 998 | 998 | 998 |
| Bore x stroke [mm] | 71.0 x 75.6 | 71 x 84 | 71 x 84 | 71 x 84 |
| Compression ratio | 11 | 10.5 | 10.5 | 10.5 |
| Maximum power [ps/rpm]  | 84 / 6,000 | 83 / 6,000 | 100 / 4,500 ~ 6,000 | 100 / 4,500 ~ 6,000 | 120 / 6,000 |
| Maximum torque [kgf·m/rpm] | 12 / 4,200 | 11.7 / 4,200 | 17.5 / 1,500~4,000 | 17.5 / 1,500~4,000 | 17.5 / 1,500~4,000 |
| Transmission | 5MT | 6MT  | 7DCT | 6iMT | 7DCT | 6iMT | 7DCT |
| 0-100 km/h [s] | 13.5 | 10.7 | 11.7 | 10.7  | 11.7 | 10.4 | 10.4 |
| Top speed [km/h]  | 165 | 183 | 180 | 183 | 180 | 185 | 185 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Weight  | 1.2 MPi | 1.0 T-GDi 100 PS  | 1.0 T-GDi 100 PS 48V  | 1.0 T-GDi 120 PS 48V  |
| Kerb weight [kg]  | 1,045/1,155 | 1,095 / 1,205 | 1,120 / 1,230 | 1,120 / 1,230 | 1,145 / 1,255 | 1,120 / 1,230 | 1,145 / 1,255 |
| Payload [kg]  | 425 / 535 | 425 / 535 | 430 / 540 | 430 / 540 | 425 / 535 | 430 / 540 | 425 / 535 |
| Gross vehicle weight [kg]  | 1580 | 1630 | 1660 | 1660 | 1680 | 1660 | 1680 |

|  |  |
| --- | --- |
| Dimensions exterior |  |
| Overall length [mm] | 4,180 |
| Overall width [mm] | 1,775 |
| Overall height [mm] |  1,490 ( 1,500with 17-inch rims) |
| Wheelbase [mm] | 2,580 |
| Wheel tread front [mm] 15-/16-/17-inch wheels | 1,551 (1,545, 1,546) |
| Wheel tread rear [mm] 15-/16-/17-inch wheels | 1,557 (1,551, 1,552) |
| Front overhang/ rear overhang [mm]  | 820 / 780 |
| Ground clearance [mm] | 165 (183 with 17-inch rims) |

|  |  |
| --- | --- |
| Dimensions interior  |  |
| Head room front/rear [mm]  | 993 / 977 |
| Leg room front/rear [mm]  | 1,072 / 882 |
| Shoulder room front/rear [mm] | 1,395 / 1,390 |
| Hip Room | 1,352 / 1,316 |

|  |  |
| --- | --- |
| Hyundai Bayon | Technical Specifications\* |

|  |  |
| --- | --- |
| Luggage Capacity |  |
| Luggage capacity VDA [l] - seats up | 411 |
| Luggage capacity VDA [l] - seats down | 1,205 |

|  |  |
| --- | --- |
| Chassis |  |
| Front suspension | McPherson Strut |
| Rear suspension | Coupled Torsion Beam Axle |
| Steering type | Gear Box: Rack & Pinion Type / MDPS: Column Type |
| Steering gear ratio  | 13.0 @20˚10.7 @360˚12.3 @360˚ AVG |
| Steering wheel lock to lock turns | 2.4 |
| Minimum turning radius [m] | 5.2 |
| Front Brake system | Ventilated Disc |
| Rear Brake system | Solid Disc |
| Front brakes diameter [mm] | 15-inch: 280 X 22T |
| Rear brakes diameter [mm] | 14-inch: 262 X 10T |
| ABS | Yes |
| Wheels | 15-inch steel / 16-inch alloy / 17-inch alloy |
| Tyres | 185/65R15, 195/55R16, 205/55R17 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Transmission | 1.2 MPi | 1.0 T-GDi 100 PS  | 1.0 T-GDi 100 PS 48V  | 1.0 T-GDi 120 PS 48V  |
| Transmission type | 5MT | 6MT  | 7DCT | 6iMT | 7DCT | 6iMT | 7DCT |
| 1st Gear :1 | 3.727 | 3.615 | 3.813[-17IN] / 3.933[+17IN]  | 3.615 | 3.813[-17IN] / 3.933[+17IN]  | 3.615 | 3.813[-17IN] / 3.933[+17IN]  |
| 2nd Gear :1 | 2.056 | 1.955 | 2.261[-17IN] / 2.381[+17IN]  | 1.955 | 2.261[-17IN] / 2.381[+17IN]  | 1.955 | 2.261[-17IN] / 2.381[+17IN]  |
| 3rd Gear :1 | 1.269 | 1.286 | 1.913[-17IN] /2.143[+17IN]  | 1.286 | 1.913[-17IN] /2.143[+17IN]  | 1.286 | 1.913[-17IN] /2.143[+17IN]  |
| 4th Gear :1 | 0.964 | 0.971 | 1.023[-17IN] / 1.128[+17IN]  | 0.971 | 1.023[-17IN] / 1.128[+17IN]  | 0.971 | 1.023[-17IN] / 1.128[+17IN]  |
| 5th Gear :1 | 0.774 | 0.794 | 0.791[-17IN] / 0.860[+17IN]  | 0.794 | 0.791[-17IN] / 0.860[+17IN]  | 0.794 | 0.791[-17IN] / 0.860[+17IN]  |
| 6th Gear :1 | - | 0.667 | 0.837[-17IN] / 0.923[+17IN]  | 0.667 | 0.837[-17IN] / 0.923[+17IN]  | 0.667 | 0.837[-17IN] / 0.923[+17IN]  |
| 7th Gear :1 | - | - | 0.690[-17IN] / 0.756[+17IN]  | - | 0.690[-17IN] / 0.756[+17IN]  | - | 0.690[-17IN] / 0.756[+17IN]  |
| Reverse :1 | 3.636 | 3.700 | 5.101[-17IN] /5.448[+17IN]  | 3.700 | 5.101[-17IN] /5.448[+17IN]  | 3.700 | 5.101[-17IN] /5.448[+17IN]  |
| Final gear ratio :1 | 4.800 | 4.059[-17IN TIRE]4.267[+17IN TIRE]" | 4.867/3.650[-17IN]4.929/3.632[+17IN] | 4.059[-17IN TIRE]4.267[+17IN TIRE] | 4.867/3.650[-17IN]4.929/3.632[+17IN] | 4.267[-17IN TIRE]4.563[+17IN TIRE] | 4.867/3.650[-17IN]4.929/3.632[+17IN] |

\*1st, 2nd, 4th, 5th gear / \*\*3rd, 6th, 7th, Reverse

ACS: Altitude Compensate System

|  |  |
| --- | --- |
| Hyundai Bayon | Technical Specifications\* |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Consumption & emissions | 1.2 MPi | 1.0 T-GDi 100 PS | 1.0 T-GDi 100 PS 48V | 1.0 T-GDi 120 PS 48V |
| Transmission type | 5MT | 6MT  | 7DCT | 6iMT | 7DCT | 6iMT | 7DCT |
| CO2 emissions combined NEDC 2.0 (g/km)\*\* high-low | 121-126 | 109-112 | 106-107 | 101-103 | 101-102 | 102-104 | TBC |
| CO2 emissions combined WLTP (g/km)\*\* high-low | 134-143 | 122-134 | 124-130 | 118-130 | 120-126 | 119-131 | TBC |

|  |
| --- |
| Notes |
| **\*** All technical specifications are tentative and subject to final homologation.\*\* CO2 emissions figures provided in this document is tentative and subject to final homologation.**Technical specifications listed in this document may vary depending on region and trim.** |